### uVision2 Project, (C) Keil Software
### Do not modify !

Target (Target 1), 0x0004 // Tools: 'ARM-ADS'

Group (USER)
Group (HARDWARE)
Group (SYSTEM)
Group (CORE)
Group (FWLib)

File 1,1,<.\main.c><main.c>
File 1,1,<.\stm32f10x_it.c><stm32f10x_it.c>
File 1,1,<.\system_stm32f10x.c><system_stm32f10x.c>
File 2,1,<..\HARDWARE\LED\led.c><led.c>
File 2,1,<..\HARDWARE\KEY\key.c><key.c>
File 2,1,<..\HARDWARE\LCD\lcd.c><lcd.c>
File 2,1,<..\HARDWARE\IIC\myiic.c><myiic.c>
File 2,1,<..\HARDWARE\24CXX\24cxx.c><24cxx.c>
File 2,1,<..\HARDWARE\SPI\spi.c><spi.c>
File 2,1,<..\HARDWARE\FLASH\flash.c><flash.c>
File 2,1,<..\HARDWARE\TOUCH\touch.c><touch.c>
File 3,1,<..\SYSTEM\delay\delay.c><delay.c>
File 3,1,<..\SYSTEM\sys\sys.c><sys.c>
File 3,1,<..\SYSTEM\usart\usart.c><usart.c>
File 4,1,<..\CORE\core_cm3.c><core_cm3.c>
File 4,2,<..\CORE\startup_stm32f10x_hd.s><startup_stm32f10x_hd.s>
File 5,1,<..\STM32F10x_FWLib\src\misc.c><misc.c>
File 5,1,<..\STM32F10x_FWLib\src\stm32f10x_fsmc.c><stm32f10x_fsmc.c>
File 5,1,<..\STM32F10x_FWLib\src\stm32f10x_gpio.c><stm32f10x_gpio.c>
File 5,1,<..\STM32F10x_FWLib\src\stm32f10x_rcc.c><stm32f10x_rcc.c>
File 5,1,<..\STM32F10x_FWLib\src\stm32f10x_spi.c><stm32f10x_spi.c>
File 5,1,<..\STM32F10x_FWLib\src\stm32f10x_usart.c><stm32f10x_usart.c>


Options 1,0,0  // Target 'Target 1'
 Device (STM32F103ZE)
 Vendor (STMicroelectronics)
 Cpu (IRAM(0x20000000-0x2000FFFF) IROM(0x8000000-0x807FFFF) CLOCK(8000000) CPUTYPE("Cortex-M3"))
 FlashUt ()
 StupF ("STARTUP\ST\STM32F10x.s" ("STM32 Startup Code"))
 FlashDR (UL2CM3(-O14 -S0 -C0 -N00("ARM Cortex-M3") -D00(1BA00477) -L00(4) -FO7 -FD20000000 -FC800 -FN1 -FF0STM32F10x_512 -FS08000000 -FL080000))
 DevID (4216)
 Rgf (stm32f10x_lib.h)
 Mem ()
 C ()
 A ()
 RL ()
 OH ()
 DBC_IFX ()
 DBC_CMS ()
 DBC_AMS ()
 DBC_LMS ()
 UseEnv=0
 EnvBin ()
 EnvInc ()
 EnvLib ()
 EnvReg (ST\STM32F10x\)
 OrgReg (ST\STM32F10x\)
 TgStat=16
 OutDir (..\OBJ\)
 OutName (TOUCH)
 GenApp=1
 GenLib=0
 GenHex=1
 Debug=1
 Browse=1
 LstDir (.\)
 HexSel=1
 MG32K=0
 TGMORE=0
 RunUsr 0 0 <>
 RunUsr 1 0 <>
 BrunUsr 0 0 <>
 BrunUsr 1 0 <>
 CrunUsr 0 0 <>
 CrunUsr 1 0 <>
 SVCSID <>
 GLFLAGS=1790
 ADSFLGA { 243,31,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ACPUTYP ("Cortex-M3")
 RVDEV ()
 ADSTFLGA { 0,12,0,2,99,0,0,66,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCMADSOCM { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCMADSIRAM { 0,0,0,0,32,0,0,1,0 }
 OCMADSIROM { 1,0,0,0,8,0,0,8,0 }
 OCMADSXRAM { 0,0,0,0,0,0,0,0,0 }
 OCR_RVCT { 1,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,1,0,0,0,8,0,0,8,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,32,0,0,1,0,0,0,0,0,0,0,0,0,0 }
 RV_STAVEC ()
 ADSCCFLG { 5,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSCMISC ()
 ADSCDEFN (STM32F10X_HD,USE_STDPERIPH_DRIVER)
 ADSCUDEF ()
 ADSCINCD (..\HARDWARE\LED;..\SYSTEM\delay;..\SYSTEM\sys;..\SYSTEM\usart;..\USER;..\STM32F10x_FWLib\inc;..\CORE;..\HARDWARE\KEY;..\HARDWARE\LCD;..\HARDWARE\RTC;..\HARDWARE\RTC;..\HARDWARE\WKUP;..\HARDWARE\ADC;..\HARDWARE\DAC;..\HARDWARE\DMA;..\HARDWARE\IIC;..\HARDWARE\24CXX;..\HARDWARE\SPI;..\HARDWARE\FLASH;..\HARDWARE\TOUCH)
 ADSASFLG { 1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSAMISC ()
 ADSADEFN ()
 ADSAUDEF ()
 ADSAINCD ()
 PropFld { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IncBld=1
 AlwaysBuild=0
 GenAsm=0
 AsmAsm=0
 PublicsOnly=0
 StopCode=3
 CustArgs ()
 LibMods ()
 ADSLDFG { 17,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 ADSLDTA (0x08000000)
 ADSLDDA (0x20000000)
 ADSLDSC ()
 ADSLDIB ()
 ADSLDIC ()
 ADSLDMC ()
 ADSLDIF ()
 ADSLDDW ()
  OPTDL (SARMCM3.DLL)()(DARMSTM.DLL)(-pSTM32F103ZE)(SARMCM3.DLL)()(TARMSTM.DLL)(-pSTM32F103ZE)
  OPTDBG 48126,7,()()()()()()()()()() (Segger\JL2CM3.dll)()()()
 FLASH1 { 9,0,0,0,1,0,0,0,5,16,0,0,0,0,0,0,0,0,0,0 }
 FLASH2 (Segger\JL2CM3.dll)
 FLASH3 ("" ())
 FLASH4 ()
EndOpt

