Static Call Graph - [..\OBJ\TOUCH.axf]

# Static Call Graph for image ..\OBJ\TOUCH.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 713]: Last Updated: Wed Dec 03 14:37:08 2014

### Maximum Stack Usage = 280 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ jiance ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TP_Adjust from touch.o(.text) referenced from touch.o(.data)
  - TP_Init from touch.o(.text) referenced from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> _fp_init
  [Called By]
  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_li ⇒ __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ jiance ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Load_Drow_Dialog (Thumb, 64 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = Load_Drow_Dialog ⇒ LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_ShowString
  - >> LCD_Clear
  [Called By]
  - >> main
  - >> jiance

  xianshi (Thumb, 132 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = xianshi ⇒ LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> showhanzi32
  - >> showhanzi16
  - >> LCD_ShowString
  [Called By]
  - >> main
  - >> refshow

  showqq (Thumb, 60 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = showqq ⇒ showimage ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> showimage
  [Called By]
  - >> main
  - >> refshow

  refshow (Thumb, 78 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = refshow ⇒ xianshi ⇒ LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_Clear
  - >> showqq
  - >> xianshi
  [Called By]
  - >> jiance

  jiance (Thumb, 64 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 280
  - Call Chain = jiance ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> TP_Save_Adjdata
  - >> TP_Adjust
  - >> LCD_Clear
  - >> refshow
  - >> Load_Drow_Dialog
  [Called By]
  - >> main

  beepms (Thumb, 30 bytes, Stack size 8 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> delay_ms

  main (Thumb, 254 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 280
  - Call Chain = main ⇒ jiance ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> uart_init
  - >> delay_init
  - >> TP_Draw_Big_Point
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> NVIC_Configuration
  - >> LED_Init
  - >> LCD_Init
  - >> LCD_Clear
  - >> KEY_Scan
  - >> KEY_Init
  - >> jiance
  - >> showqq
  - >> xianshi
  - >> Load_Drow_Dialog
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 82 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 154 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  LED_Init (Thumb, 102 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Init (Thumb, 60 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Scan (Thumb, 196 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = KEY_Scan
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> main

  LCD_WR_REG (Thumb, 40 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_REG
  [Calls]
  - >> SPI_WriteByte
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_REG_DATA
  - >> LCD_Init

  LCD_WR_DATA (Thumb, 48 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_DATA
  [Calls]
  - >> SPI_WriteByte
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> LCD_WR_REG_DATA
  - >> showimage
  - >> showhanzi32
  - >> showhanzi16
  - >> LCD_Clear

  LCD_WR_DATA8 (Thumb, 40 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_DATA8
  [Calls]
  - >> SPI_WriteByte
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_WR_REG_DATA (Thumb, 20 bytes, Stack size 16 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WR_DATA
  - >> LCD_WR_REG

  LCD_WriteRAM_Prepare (Thumb, 12 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WriteRAM_Prepare ⇒ LCD_WR_REG
  [Calls]
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> showimage
  - >> showhanzi32
  - >> showhanzi16
  - >> LCD_Clear

  opt_delay (Thumb, 14 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)

  LCD_DisplayOn (Thumb, 2 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)

  LCD_DisplayOff (Thumb, 2 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)

  LCD_SetCursor (Thumb, 48 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_WR_DATA8
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> showimage
  - >> showhanzi32
  - >> showhanzi16
  - >> LCD_Clear

  LCD_DrawPoint (Thumb, 28 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_ShowChar
  - >> Draw_Circle
  - >> LCD_DrawLine
  - >> TP_Draw_Big_Point

  LCD_Clear (Thumb, 50 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> TP_Adjust
  - >> LCD_Init
  - >> main
  - >> jiance
  - >> refshow
  - >> Load_Drow_Dialog

  LCD_Init (Thumb, 612 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_Init ⇒ LCD_Clear ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_WR_DATA8
  - >> LCD_WR_REG
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> main

  LCD_Fill (Thumb, 120 bytes, Stack size 40 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA

  LCD_Color_Fill (Thumb, 104 bytes, Stack size 40 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare

  LCD_DrawLine (Thumb, 190 bytes, Stack size 72 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 64 bytes, Stack size 24 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  Draw_Circle (Thumb, 170 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = Draw_Circle ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point

  showhanzi16 (Thumb, 124 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = showhanzi16 ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> xianshi

  showhanzi32 (Thumb, 124 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = showhanzi32 ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> xianshi

  LCD_ShowChar (Thumb, 390 bytes, Stack size 40 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum
  - >> LCD_ShowString

  LCD_Pow (Thumb, 24 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Pow
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 156 bytes, Stack size 56 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show

  LCD_ShowxNum (Thumb, 202 bytes, Stack size 64 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_Pow
  - >> LCD_ShowChar

  LCD_ShowString (Thumb, 106 bytes, Stack size 40 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show
  - >> TP_Adjust
  - >> xianshi
  - >> Load_Drow_Dialog

  showimage (Thumb, 102 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = showimage ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> showqq

  SPI1_Init (Thumb, 260 bytes, Stack size 32 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI1_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_ResetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  SPI2_ReadWriteByte (Thumb, 86 bytes, Stack size 16 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI2_ReadWriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SPI_Flash_WAKEUP
  - >> SPI_Flash_PowerDown
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page
  - >> SPI_Flash_Read
  - >> SPI_FLASH_Write_Disable
  - >> SPI_FLASH_Write_Enable
  - >> SPI_FLASH_Write_SR
  - >> SPI_Flash_ReadSR
  - >> SPI_Flash_ReadID
  - >> SPI2_Init

  SPI2_Init (Thumb, 160 bytes, Stack size 32 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB1PeriphClockCmd
  - >> SPI2_ReadWriteByte
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> SPI_Flash_Init

  SPI2_SetSpeed (Thumb, 42 bytes, Stack size 8 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI2_SetSpeed
  [Calls]
  - >> SPI_Cmd
  [Called By]
  - >> SPI_Flash_Init

  SPI_WriteByte (Thumb, 30 bytes, Stack size 0 bytes, spi.o(.text))
  [Called By]

  - >> LCD_WR_DATA8
  - >> LCD_WR_DATA
  - >> LCD_WR_REG

  SPI_Flash_ReadID (Thumb, 74 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_Flash_ReadID ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Init

  SPI_Flash_Init (Thumb, 122 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = SPI_Flash_Init ⇒ SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Flash_ReadID
  - >> SPI2_SetSpeed
  - >> SPI2_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  SPI_Flash_ReadSR (Thumb, 42 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Wait_Busy

  SPI_FLASH_Write_SR (Thumb, 38 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI2_ReadWriteByte

  SPI_FLASH_Write_Enable (Thumb, 30 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_FLASH_Write_Enable ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page

  SPI_FLASH_Write_Disable (Thumb, 30 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI2_ReadWriteByte

  SPI_Flash_Read (Thumb, 84 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_Flash_Read ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> TP_Get_Adjdata
  - >> SPI_Flash_Write

  SPI_Flash_Wait_Busy (Thumb, 18 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_ReadSR
  [Called By]
  - >> SPI_Flash_Erase_Chip
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_Page

  SPI_Flash_Write_Page (Thumb, 90 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Write_NoCheck

  SPI_Flash_Write_NoCheck (Thumb, 72 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Write_Page
  [Called By]
  - >> SPI_Flash_Write

  SPI_Flash_Erase_Sector (Thumb, 70 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SPI_Flash_Erase_Sector ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> SPI_Flash_Write

  SPI_Flash_Write (Thumb, 186 bytes, Stack size 32 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Erase_Sector
  - >> SPI_Flash_Write_NoCheck
  - >> SPI_Flash_Read
  [Called By]
  - >> TP_Save_Adjdata

  SPI_Flash_Erase_Chip (Thumb, 42 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI_Flash_Wait_Busy
  - >> SPI_FLASH_Write_Enable
  - >> SPI2_ReadWriteByte

  SPI_Flash_PowerDown (Thumb, 38 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI2_ReadWriteByte
  - >> delay_us

  SPI_Flash_WAKEUP (Thumb, 38 bytes, Stack size 8 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> SPI2_ReadWriteByte
  - >> delay_us

  TP_Write_Byte (Thumb, 70 bytes, Stack size 0 bytes, touch.o(.text))
  [Called By]

  - >> TP_Read_AD

  TP_Read_AD (Thumb, 140 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TP_Read_AD
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 158 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 40 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Init
  - >> TP_Read_XY2

  TP_Read_XY2 (Thumb, 198 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 110 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = TP_Drow_Touch_Point ⇒ LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> Draw_Circle
  - >> LCD_DrawLine
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 54 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Draw_Big_Point ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> main

  TP_Scan (Thumb, 294 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY2
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fadd
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 138 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = TP_Save_Adjdata ⇒ SPI_Flash_Write ⇒ SPI_Flash_Write_NoCheck ⇒ SPI_Flash_Write_Page ⇒ SPI_Flash_Wait_Busy ⇒ SPI_Flash_ReadSR ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Write
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  [Called By]
  - >> TP_Adjust
  - >> jiance

  TP_Get_Adjdata (Thumb, 192 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Get_Adjdata ⇒ SPI_Flash_Read ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI_Flash_Read
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 382 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 184
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> LCD_ShowNum
  - >> LCD_ShowString
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 2168 bytes, Stack size 88 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 272
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA8
  [Calls]
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Drow_Touch_Point
  - >> delay_ms
  - >> TP_Save_Adjdata
  - >> LCD_ShowString
  - >> LCD_Clear
  - >> sqrt
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_f2iz
  - >> __aeabi_fdiv
  - >> __aeabi_fsub
  - >> __aeabi_f2d
  [Called By]
  - >> jiance
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 114 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = TP_Init ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Get_Adjdata
  - >> TP_Read_XY
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  delay_init (Thumb, 42 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 76 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> TP_Read_AD
  - >> SPI_Flash_WAKEUP
  - >> SPI_Flash_PowerDown

  delay_ms (Thumb, 76 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> TP_Adjust
  - >> LCD_Init
  - >> KEY_Scan
  - >> beepms

  NVIC_Configuration (Thumb, 12 bytes, Stack size 8 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_Configuration
  [Calls]
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  inttohex (Thumb, 136 bytes, Stack size 8 bytes, sys.o(.text), UNUSED)

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 20 bytes, Stack size 0 bytes, usart.o(.text), UNUSED)

  uart_init (Thumb, 176 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_Cmd
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 128 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 292 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> TP_Init
  - >> SPI2_Init
  - >> uart_init
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> LED_Init
  - >> KEY_Init

  GPIO_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> KEY_Scan

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> SPI2_Init
  - >> LCD_WR_DATA8
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> SPI_Flash_Init
  - >> LED_Init
  - >> LCD_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LCD_WR_DATA8
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> SPI1_Init
  - >> LED_Init
  - >> LCD_Init

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 156 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 84 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 68 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 68 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 36 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 216 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> I2S_Init
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> TP_Init
  - >> SPI2_Init
  - >> uart_init
  - >> SPI_Flash_Init
  - >> SPI1_Init
  - >> LED_Init
  - >> KEY_Init

  RCC_APB1PeriphClockCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI2_Init

  RCC_APB2PeriphResetCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit
  - >> USART_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 58 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 80 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI2_Init
  - >> SPI1_Init

  I2S_Init (Thumb, 250 bytes, Stack size 56 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_SetSpeed
  - >> SPI2_Init
  - >> SPI1_Init

  I2S_Cmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 50 bytes, Stack size 16 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_ReadWriteByte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_ReadWriteByte

  SPI_NSSInternalSoftwareConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_ReadWriteByte

  SPI_I2S_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 68 bytes, Stack size 20 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 28 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> uart_init

  USART_Init (Thumb, 250 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_StructInit (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 46 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_ITConfig (Thumb, 88 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_DMACmd (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 54 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 104 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 40 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 12 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 128 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init

  NVIC_SetVectorTable (Thumb, 16 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 30 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> sqrt

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __rt_fp_status_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_fp_status_addr_intlibspace.o(.text))
  [Called By]

  - >> _fp_init

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> TP_Adjust

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> TP_Adjust

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> TP_Adjust

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dcmple
  - >> _dfixu
  - >> _dsqrt

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> TP_Adjust

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> TP_Adjust

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_fadd (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fadd
  [Called By]
  - >> TP_Scan

  _fadd (Thumb, 196 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf
  - >> _fsub1

  __aeabi_fdiv (Thumb, 0 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Called By]
  - >> TP_Get_Adjdata
  - >> TP_Adjust

  _fdiv (Thumb, 384 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_f2iz (Thumb, 0 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2iz
  [Called By]
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _ffix (Thumb, 54 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> TP_Scan
  - >> TP_Adjust

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_i2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt))
  [Called By]

  - >> TP_Get_Adjdata
  - >> TP_Scan
  - >> TP_Adjust

  _fflt (Thumb, 48 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt), UNUSED)

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> TP_Scan
  - >> TP_Adjust

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __aeabi_fmul (Thumb, 0 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Scan
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _fmul (Thumb, 258 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _ffixu
  - >> _ffix
  - >> _fdiv
  - >> _fsub
  - >> _fadd
  - >> _f2d

  _fp_init (Thumb, 14 bytes, Stack size 8 bytes, fpinit.o(x$fpl$fpinit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _fp_init
  [Calls]
  - >> __rt_fp_status_addr
  [Called By]
  - >> __rt_lib_init

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fdiv
  - >> _fadd

  __aeabi_fsub (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fsub
  [Called By]
  - >> TP_Adjust

  _fsub (Thumb, 234 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> _fadd1

  __I$use$fp (Thumb, 0 bytes, Stack size unknown bytes, usenofp.o(x$fpl$usenofp), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 200 bytes, Stack size 0 bytes, system_stm32f10x.o(.text))
  [Called By]

  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetSysClock
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  _fadd1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Called By]

  - >> _fsub

  _fsub1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Called By]

  - >> _fadd

  ### Undefined Global Symbols